Low standard vs detection limit

Laboratory blanks. QAC/BLK/DI/LAB, try to keep it under 10

Autosampler 181 is always DI. A zero is always included in the standard curver

Lab std checks are all good.

Have Pegasus person consult with Dana regarding analytical schedule component of Lachat sample submission form.